Mikrotik Stup

Hosting Internal server

IP > Firewall > NAT : We can specify our own server for external access.

8181 - This is to MAC mini server Time log and mSupply registration page.

5900 -- This is to MAC mini screenshare

9100 -- This is to the label printer 192.168.3.246 for Moneyworks staff to do some label printing

NAT list

Setting for port 8181

Domain re-direct

IP > DNS > Static button

We can re-point ktm.msupply.org to our mac mini server : 192.168.3.200

DHCP Server

IP > DHCP Server > Lease : We can lease IP address to a hardware